1. Default baud rate is 115200, N, 8, 1.

2. module contains tow MAC address, 00:0E:0B:xx:xx:xx is BLE mode, 00:0E:0E:xx:xx:xx is EDR mode.

3. Our company provides two version bluetooth serial assistant, BLE Comassistant and SPP ComAssistant.

4. Dont iperate the BLE in android Bluetooth management interface¡£

5. Before V216 PIO0 must pull up¡£

6. Since V216 you can shut down PIO0 function use AT+PIO0 command. After execute AT+PIO00 command, you can left PIO0 NC.

7. Since V216 we setup AT+MODE1 as default settings.

8. Query version command is AT+VERS?

9. The AT command is uppercase characters, dont have any other symbols.

A. Dual mode module dont have high speed, Please make some delay time between two packages.


